<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<description>&lt;b&gt;Mini PCI-Express Card&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by chris@hobbyelektronik.org&lt;/author&gt;

&lt;br&gt;&lt;br&gt;
Used PCI-SIG Specs 1.0 with addiotional information from http://www.allpinouts.org/index.php/PCI_Express_Card_and_PCI_Express_Mini_Card

&lt;br&gt;&lt;br&gt;
Made with best knowledge and conscience but errors not excluded. Please report all flaws to me - I don't want to grill any notebook.

&lt;br&gt;&lt;br&gt;

&lt;b&gt;Additional information&lt;/b&gt;
&lt;br&gt;The PCB must be 1.0mm thick. Components on top mustn't excess a height of 2.4mm and 1.35mm on bottom!</description>
<packages>
<package name="MINI_PCIE">
</package>
<package name="MINI_PCIE_HALF">
</package>
</packages>
<symbols>
<symbol name="MINI_PCIE">
<pin name="RSVRD51"/>
<pin name="RSVRD49"/>
<pin name="RSVRD47"/>
<pin name="RSVRD45"/>
<pin name="GND@43"/>
<pin name="+3V3AUX@41"/>
<pin name="+3V3AUX@39"/>
<pin name="GND@37"/>
<pin name="GND@35" direction="pwr"/>
<pin name="PETP0"/>
<pin name="PETN0"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="PERP0"/>
<pin name="PERN0"/>
<pin name="GND@21" direction="pwr"/>
<pin name="UIM_C4"/>
<pin name="UIM_C8"/>
<pin name="GND@15" direction="pwr"/>
<pin name="REFCLK+" direction="in"/>
<pin name="REFCLK-" direction="in"/>
<pin name="GND@9" direction="pwr"/>
<pin name="CLKREQ" direction="out" function="dot"/>
<pin name="COEX2"/>
<pin name="COEX1"/>
<pin name="WAKE" direction="out" function="dot"/>
<pin name="+1V5@28" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="+3V3@52" direction="pwr"/>
<pin name="GND@50" direction="out"/>
<pin name="+1V5@48" direction="out"/>
<pin name="LED_WPAN" direction="out" function="dot"/>
<pin name="LED_WLAN" direction="out" function="dot"/>
<pin name="LED_WWAN" direction="out" function="dot"/>
<pin name="GND@40"/>
<pin name="USB_D+" direction="pwr"/>
<pin name="USB_D-"/>
<pin name="GND@34"/>
<pin name="SMB_DATA" direction="pwr"/>
<pin name="SMB_CLK" direction="in"/>
<pin name="+3V3AUX@24" direction="pwr"/>
<pin name="PERST" direction="in" function="dot"/>
<pin name="W_DISABLE" direction="in" function="dot"/>
<pin name="GND@18" direction="pwr"/>
<pin name="UIM_VPP"/>
<pin name="UIM_RESET"/>
<pin name="UIM_CLK"/>
<pin name="UIM_DATA"/>
<pin name="UIM_PWR"/>
<pin name="+1V5@6" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="+3V3@2" direction="pwr"/>
</symbol>
<symbol name="MINI_PCI_HOLES">
<pin name="GND@H1T" direction="pwr"/>
<pin name="GND@H1B" direction="pwr"/>
<pin name="GND@H2T" direction="pwr"/>
<pin name="GND@H2B" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MINI_PCIE">
<gates>
<gate name="G$1" symbol="MINI_PCIE"/>
<gate name="G$2" symbol="MINI_PCI_HOLES"/>
</gates>
<devices>
<device name="" package="MINI_PCIE">
<connects>
<connect gate="G$1" pin="+1V5@28" pad="28"/>
<connect gate="G$1" pin="+1V5@48" pad="48"/>
<connect gate="G$1" pin="+1V5@6" pad="6"/>
<connect gate="G$1" pin="+3V3@2" pad="2"/>
<connect gate="G$1" pin="+3V3@52" pad="52"/>
<connect gate="G$1" pin="+3V3AUX@24" pad="24"/>
<connect gate="G$1" pin="+3V3AUX@39" pad="39"/>
<connect gate="G$1" pin="+3V3AUX@41" pad="41"/>
<connect gate="G$1" pin="CLKREQ" pad="7"/>
<connect gate="G$1" pin="COEX1" pad="3"/>
<connect gate="G$1" pin="COEX2" pad="5"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="GND@34" pad="34"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@37" pad="37"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@40" pad="40"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="GND@50" pad="50"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="LED_WLAN" pad="44"/>
<connect gate="G$1" pin="LED_WPAN" pad="46"/>
<connect gate="G$1" pin="LED_WWAN" pad="42"/>
<connect gate="G$1" pin="PERN0" pad="23"/>
<connect gate="G$1" pin="PERP0" pad="25"/>
<connect gate="G$1" pin="PERST" pad="22"/>
<connect gate="G$1" pin="PETN0" pad="31"/>
<connect gate="G$1" pin="PETP0" pad="33"/>
<connect gate="G$1" pin="REFCLK+" pad="13"/>
<connect gate="G$1" pin="REFCLK-" pad="11"/>
<connect gate="G$1" pin="RSVRD45" pad="45"/>
<connect gate="G$1" pin="RSVRD47" pad="47"/>
<connect gate="G$1" pin="RSVRD49" pad="49"/>
<connect gate="G$1" pin="RSVRD51" pad="51"/>
<connect gate="G$1" pin="SMB_CLK" pad="30"/>
<connect gate="G$1" pin="SMB_DATA" pad="32"/>
<connect gate="G$1" pin="UIM_C4" pad="19"/>
<connect gate="G$1" pin="UIM_C8" pad="17"/>
<connect gate="G$1" pin="UIM_CLK" pad="12"/>
<connect gate="G$1" pin="UIM_DATA" pad="10"/>
<connect gate="G$1" pin="UIM_PWR" pad="8"/>
<connect gate="G$1" pin="UIM_RESET" pad="14"/>
<connect gate="G$1" pin="UIM_VPP" pad="16"/>
<connect gate="G$1" pin="USB_D+" pad="38"/>
<connect gate="G$1" pin="USB_D-" pad="36"/>
<connect gate="G$1" pin="WAKE" pad="1"/>
<connect gate="G$1" pin="W_DISABLE" pad="20"/>
<connect gate="G$2" pin="GND@H1B" pad="HOLE1B"/>
<connect gate="G$2" pin="GND@H1T" pad="HOLE1T"/>
<connect gate="G$2" pin="GND@H2B" pad="HOLE2B"/>
<connect gate="G$2" pin="GND@H2T" pad="HOLE2T"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HALF" package="MINI_PCIE_HALF">
<connects>
<connect gate="G$1" pin="+1V5@28" pad="28"/>
<connect gate="G$1" pin="+1V5@48" pad="48"/>
<connect gate="G$1" pin="+1V5@6" pad="6"/>
<connect gate="G$1" pin="+3V3@2" pad="2"/>
<connect gate="G$1" pin="+3V3@52" pad="52"/>
<connect gate="G$1" pin="+3V3AUX@24" pad="24"/>
<connect gate="G$1" pin="+3V3AUX@39" pad="39"/>
<connect gate="G$1" pin="+3V3AUX@41" pad="41"/>
<connect gate="G$1" pin="CLKREQ" pad="7"/>
<connect gate="G$1" pin="COEX1" pad="3"/>
<connect gate="G$1" pin="COEX2" pad="5"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="GND@34" pad="34"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@37" pad="37"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@40" pad="40"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="GND@50" pad="50"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="LED_WLAN" pad="44"/>
<connect gate="G$1" pin="LED_WPAN" pad="46"/>
<connect gate="G$1" pin="LED_WWAN" pad="42"/>
<connect gate="G$1" pin="PERN0" pad="23"/>
<connect gate="G$1" pin="PERP0" pad="25"/>
<connect gate="G$1" pin="PERST" pad="22"/>
<connect gate="G$1" pin="PETN0" pad="31"/>
<connect gate="G$1" pin="PETP0" pad="33"/>
<connect gate="G$1" pin="REFCLK+" pad="13"/>
<connect gate="G$1" pin="REFCLK-" pad="11"/>
<connect gate="G$1" pin="RSVRD45" pad="45"/>
<connect gate="G$1" pin="RSVRD47" pad="47"/>
<connect gate="G$1" pin="RSVRD49" pad="49"/>
<connect gate="G$1" pin="RSVRD51" pad="51"/>
<connect gate="G$1" pin="SMB_CLK" pad="30"/>
<connect gate="G$1" pin="SMB_DATA" pad="32"/>
<connect gate="G$1" pin="UIM_C4" pad="19"/>
<connect gate="G$1" pin="UIM_C8" pad="17"/>
<connect gate="G$1" pin="UIM_CLK" pad="12"/>
<connect gate="G$1" pin="UIM_DATA" pad="10"/>
<connect gate="G$1" pin="UIM_PWR" pad="8"/>
<connect gate="G$1" pin="UIM_RESET" pad="14"/>
<connect gate="G$1" pin="UIM_VPP" pad="16"/>
<connect gate="G$1" pin="USB_D+" pad="38"/>
<connect gate="G$1" pin="USB_D-" pad="36"/>
<connect gate="G$1" pin="WAKE" pad="1"/>
<connect gate="G$1" pin="W_DISABLE" pad="20"/>
<connect gate="G$2" pin="GND@H1B" pad="HOLE1B"/>
<connect gate="G$2" pin="GND@H1T" pad="HOLE1T"/>
<connect gate="G$2" pin="GND@H2B" pad="HOLE2B"/>
<connect gate="G$2" pin="GND@H2T" pad="HOLE2T"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
